**UNITED METHODIST COMMITTEE ON RELIEF (UMCOR) HAITI**

**TENDER NOTICE**

 **Supply of Items/Material for construction of Latrines**

**Background:-**

UMCOR’s Haiti mission is to provide emergency response, early recovery and transitional development assistance having long history of working in Haiti. **UMCOR** is implementing integrated program in the Municipality of Tabarre, Thomazeau and Cabaret. The overall goal of the Water, sanitation and Hygiene (WASH***)*** programis to address and facilitate the communities concerning health, sanitation & hygiene issues through variety of interventions. In order to promote sanitation in communities of the West department **UMCOR** intends to initiate construction of latrines in identified schools; **UMCOR** Haiti seeks service provider/ contractor for providing items mentioned in table. The service provider/ contractor will be responsible to deliver high-quality items with specification based on details provided in table.

**Description:-**

United Methodist Committee on Relief (UMCOR) Haiti invites sealed Bids from reputed and eligible firms/contractors/Organizations/ preferably registered from relevant Ministry/ Department/ DGI office. Applying contractors must have strong financial and alike technical background to deliver required items/ materials within agreed time frame of project to avoid any unexpected delay.

**Deliverables: -**Service provider/vendor is responsible to deliver required items/material in accordance with specification stated in table underneath.

**Submission of Bids: -**The contractors are requested to submit sealed Bids before: ***12:00 pm 15th of July, 2016***. It is pertinent that bids should be submitted in **English.**

 **Bids Opening:** Contractors are invited to the bid opening which will be at: UMCOR, s Port-au-Prince office at: ***2:00 pm 15thof July, 2016***

The bids must include:

1. Completed Items including unit costs as well as cumulative budget. These should include all costs, including items and transport to project site.

Bids can be submitted in a sealed envelope to the following address:

**UNITED METHODIST COMMITTEE on RELIEF (HAITI)**

**P.O Box 15562,HT 6140, Port- au-Prince, Haïti, Or** Sealed bids can be submitted by hand at **16, Delmas 54 office UMCOR-Haiti**

(Separate box is designated for submission of Bids),

For question & clarification, please contact: ***procurement@umcor-haiti.org***

**Bids Evaluation:-**

The evaluation of bids will be carried out in accordance with defined policies and procedures of UMCOR. There will be evaluation of technical bids which represent 60% of the points and followed by evaluation of financial bids which represent 40% of the points.

**Refusal of Bids:-**

 UMCOR Haiti reserves the right to cancel tender process or to reject all bids without any liability to bidders. UMCOR Haiti has no liability of payment incurred for documentation of bids/transportation and any other relevant cost incurred during process of submission of bids from vendors/contractors.

**Note: -** Bids submitted electronically will be considered in-eligible for process.

 ***\* Please separate Aggregates from Materials***

|  |  |  |  |
| --- | --- | --- | --- |
| **Items #** | **Description Specification / Brand** | **total Quantity** | **Unit / Measure** |
| **AGGREGATES** |
| 1 | blocks # 20 | 3000 | Unit |
| 2 |  blocks # 15 | 2600 | unit |
| 3 | blocks #10 | 280 | unit |
| 4 | Sable lave | 140 | M3 |
| 5 | Gravel 12/25 | 40 | M3 |
| 6 | Remblais | 28 | M3 |
| **MATERIALS** |
| 1 | Ciment  | 1000 | sac |
| 2 | Fer 1/2 | 440 | rebar |
| 3 | fer 3/8 | 480 | rebar |
| 4 | Fil a ligature | 400 | lb |
| 5 | Bois 2x4x16 | 120 | Unit |
| 6 | Bois1x12x16 | 24 | Unit |
| 7 | Plywood 3/4 | 24 | Unit |
| 8 | planche | 48 | unit |
| 9 | clous 3'' | 8 | broit |
| 10 | bois dur | 12 | dz |
| 11 | tuyaux 4''sch-40 | 36 | Unit |
| 12 | tole trapezoidale Rouge | 32 | unt |
| 13 | profile 2x2 | 36 | unt |
| 14 | profile1x2 | 36 | unt |
| 15 | minium  | 12 | gal |
| 16 | accord  | 24 | Unit |
| 17 | vise tole  | 480 | unt  |
| 18 | Ceremique anti derapente | 100 | m2 |
| 19 | Peiture (semie Glose) Grise | 60 | Gal |
| 20 | Robinet a Poussoir temporise | 20 | PC |
| 21 | Sablé pour mur (#1 et #2) | 24 | Feuille |